/** \file
 *
 *  This file contains special DoxyGen information for the generation of the main page and other special
 *  documentation pages. It is not a project source file.
 */
 
/** \mainpage Joystick Device Demo
 *
 *  \section SSec_Compat Demo Compatibility:
 *
 *  The following table indicates what microcontrollers are compatible with this demo.
 *
 *  - AT90USB1287
 *  - AT90USB1286
 *  - AT90USB647
 *  - AT90USB646
 *  - ATMEGA32U6
 *  - ATMEGA32U4
 *  - ATMEGA16U4
 *  - AT90USB162
 *  - AT90USB82
 *
 *  \section SSec_Info USB Information:
 *
 *  The following table gives a rundown of the USB utilization of this demo.
 *
 *  <table>
 *   <tr>
 *    <td><b>USB Mode:</b></td>
 *    <td>Device</td>
 *   </tr>
 *   <tr>
 *    <td><b>USB Class:</b></td>
 *    <td>Human Interface Device (HID)</td>
 *   </tr>
 *   <tr> 
 *    <td><b>USB Subclass:</b></td>
 *    <td>N/A</td>
 *   </tr>
 *   <tr>
 *    <td><b>Relevant Standards:</b></td>
 *    <td>USBIF HID Specification, USBIF HID Usage Tables</td>
 *   </tr>
 *   <tr>
 *    <td><b>Usable Speeds:</b></td>
 *    <td>Low Speed Mode, Full Speed Mode</td>
 *   </tr>
 *  </table>
 *
 *  \section SSec_Description Project Description: 
 *
 *  Joystick demonstration application. This gives a simple reference
 *  application for implementing a USB Keyboard device, for USB Joysticks
 *  using the standard Keyboard HID profile.
 *  
 *  This device will show up as a generic joystick device, with two buttons.
 *  Pressing the joystick inwards is the first button, and the HWB button
 *  is the second.
 *  
 *  Moving the joystick on the selected board moves the joystick location on
 *  the host computer.
 *  
 *  Currently only single interface joysticks are supported.
 *
 *  \section SSec_Options Project Options
 *
 *  The following defines can be found in this demo, which can control the demo behaviour when defined, or changed in value.
 *
 *  <table>
 *   <tr>
 *    <td>
 *     None
 *    </td>
 *   </tr>
 *  </table>
 */